{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["工程量清单","练湖新城","紫竹园"],"read":"whole","date_system":"1900"}

{"sheet":"工程量清单","index":0,"n_rows":8,"n_cols":3,"rows_kept":8}
["项目名称","项目特征描述","工程量（平方米）"]
["屋面卷材防水","1、卷材品种、规格、厚度：4mm厚SBS改性沥青防水卷材\n2、防水层做法：聚氨酯防水涂料厚1.5mm；4mm厚SBS改性沥青防水卷材防水层",1476.73]
["铲除涂料面","1、铲除部位名称：外墙涂料",2117.44]
["墙面喷刷涂料","1、基层类型：外墙面\n2、喷刷涂料部位：外墙面\n3、腻子种类：901胶白水泥腻子\n4、刮腻子要求：二遍\n5、涂料品种、喷刷遍数：外墙乳胶漆毛面",2029.42]
["飘窗水泥砂浆找平层拆除","1、部位：飘窗板\n2、找平层厚度：20厚水泥砂浆",88.02]
["屋面刚性层","1、部位：飘窗板\n2、刚性层厚度：20厚1：2防水砂浆",88.02]
["屋面涂膜防水","1、部位：飘窗板\n2、防水膜品种：聚氨酯防水涂料\n3、涂膜厚度、遍数：1.5厚两遍成形",88.02]
["外装饰吊篮",null,2296.75]

{"sheet":"练湖新城","index":1,"n_rows":326,"n_cols":5,"rows_kept":326,"merged":[[0,0,0,4],[325,2,325,4]]}
["练湖新城"]
["维修部位","长度","宽度（高度）","计量","总量"]
["B22-1-701"]
["南房南墙",3.36,6.5,1,21.84]
["飘窗",1.7,1.8,-1,-3.06]
["飘窗顶",1.7,1,1,{"v":1.7,"d":"1.70"}]
["A4-4-608"]
["西墙",2.65,21,1,55.65]
["西墙平台",4.5,3,1,{"v":13.5,"d":"13.50"}]
["南房南墙",3.45,3,1,10.35]
["窗",1.85,1.76,-1,{"v":-3.256,"d":"-3.26"}]
["南房西墙",3.93,3,1,11.79]
["北房北墙",3.06,3,1,9.18]
["窗",1.85,1.76,-1,{"v":-3.256,"d":"-3.26"}]
["北房西墙",2.9,3,1,{"v":8.7,"d":"8.70"}]
["楼道顶",2.35,4.9,1,{"v":11.515,"d":"11.52"}]
["阁楼东墙",2.04,1.88,1,{"v":3.8352,"d":"3.84"}]
["A10-3-609"]
["阁楼南墙",3.39,3,1,10.17]
["南飘窗",1.75,1.35,-1,{"v":-2.3625,"d":"-2.36"}]
["飘窗顶",1.75,1,1,1.75]
["西采光井1",3.74,3,1,11.22]
["西采光井2",1.3,1,1,{"v":1.3,"d":"1.30"}]
["楼面1",7.66,6.8,1,{"v":52.088,"d":"52.09"}]
["楼面2",4.3,1.4,1,6.02]
["围墙",7.32,0.42,1,{"v":3.0744,"d":"3.07"}]
["石墩1",0.51,0.51,-39,{"v":-10.1439,"d":"-10.14"}]
["石墩2",1.5,0.38,39,22.23]
["烟道",{"v":0.6232,"d":"0.62"},{"v":1.022,"d":"1.02"},2,{"v":1.2738208,"d":"1.27"}]
["天沟1",4.2,1,1,{"v":4.2,"d":"4.20"}]
["天沟2",3.08,1,1,3.08]
["北房北墙",3.2,4,1,{"v":12.8,"d":"12.80"}]
["北飘窗",1.75,1.35,-1,{"v":-2.3625,"d":"-2.36"}]
["飘窗顶",1.75,1,1,1.75]
["阳台顶",3.76,1.86,1,{"v":6.9936,"d":"6.99"}]
["A13-4-107"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["窗",1.87,1.78,-2,{"v":-6.6572,"d":"-6.66"}]
["飘窗顶",1.5,1,1,{"v":1.5,"d":"1.50"}]
["A13-4-108"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["窗",1.87,1.78,-2,{"v":-6.6572,"d":"-6.66"}]
["飘窗顶",1.5,1,1,{"v":1.5,"d":"1.50"}]
["北房北墙",3.2,4,1,{"v":12.8,"d":"12.80"}]
["北飘窗",1.75,1.35,-1,{"v":-2.3625,"d":"-2.36"}]
["飘窗顶",1.75,1,1,1.75]
["A13-4-508"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["窗",1.87,1.78,-2,{"v":-6.6572,"d":"-6.66"}]
["飘窗顶",1.5,1,1,{"v":1.5,"d":"1.50"}]
["A7-4-607"]
["阁楼西墙斜面",2.77,2.5,1,{"v":6.925,"d":"6.93"}]
["阁楼楼面",3.7,3.4,1,12.58]
["南天沟",3.8,2,1,{"v":7.6,"d":"7.60"}]
["A7-4-608"]
["西墙",2.65,21,1,55.65]
["西墙平台",4.5,2,1,{"v":9,"d":"9.00"}]
["阁楼西墙斜面",2.77,2.5,1,{"v":6.925,"d":"6.93"}]
["阁楼楼面",3.7,3.4,1,12.58]
["南天沟",3.8,2.5,1,{"v":9.5,"d":"9.50"}]
["北天沟",4.2,1.5,1,{"v":6.3,"d":"6.30"}]
["西天沟",3.76,0.31,1,{"v":1.1656,"d":"1.17"}]
["西平台",6.1,1.96,1,{"v":11.956,"d":"11.96"}]
["A13-4-607"]
["烟道",0.62,1.02,1,{"v":0.6324,"d":"0.63"}]
["阳台 南墙",{"v":3.5,"d":"3.50"},{"v":1,"d":"1.00"},1,{"v":3.5,"d":"3.50"}]
["A15-3-506"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["西南房西墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["空调板",1.86,1,1,1.86]
["A18-1-301"]
["东墙",2.65,21,1,55.65]
["东墙平台",4.15,2,1,{"v":8.3,"d":"8.30"}]
["南房东墙",4.25,6.5,1,{"v":27.625,"d":"27.63"}]
["A10-3-608"]
["南墙",3.36,6.5,1,21.84]
["西墙",3.09,6.5,1,{"v":20.085,"d":"20.09"}]
["飘窗顶",1.86,1,1,1.86]
["楼面1",7.4,6.33,1,{"v":46.842,"d":"46.84"}]
["楼面2",4.5,1.6,1,{"v":7.2,"d":"7.20"}]
["石墩1",0.51,0.51,-40,{"v":-10.404,"d":"-10.40"}]
["石墩2",1.5,0.38,40,{"v":22.8,"d":"22.80"}]
["阁楼东墙斜面",6,2.9,1,{"v":17.4,"d":"17.40"}]
["A19-1-501"]
["南房南墙",2.75,6.5,1,{"v":17.875,"d":"17.88"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["东南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["东南房东墙",4.25,6.5,1,{"v":27.625,"d":"27.63"}]
["厨房东墙",4.1,6.5,1,26.65]
["客厅北空调板",1.5,1,1,{"v":1.5,"d":"1.50"}]
["客厅北墙",1.2,6.5,1,{"v":7.8,"d":"7.80"}]
["东墙",2.65,21,1,55.65]
["东墙平台",4.3,2,1,{"v":8.6,"d":"8.60"}]
["卫生间北墙",1.56,6.5,1,10.14]
["A25-1-601"]
["北房北墙",2.57,3,1,7.71]
["北飘窗",1.85,1.45,-1,{"v":-2.6825,"d":"-2.68"}]
["飘窗顶",1.45,1,1,1.45]
["北房东墙",3.6,3,1,{"v":10.8,"d":"10.80"}]
["南房南墙",3.4,3,1,{"v":10.2,"d":"10.20"}]
["南飘窗",1.85,1.75,-1,{"v":-3.2375,"d":"-3.24"}]
["飘窗顶",1.75,1,1,1.75]
["南房东墙",6.65,3,1,19.95]
["窗",1.78,0.8,-1,{"v":-1.424,"d":"-1.42"}]
["南北房楼面",6.3,1.95,1,{"v":12.285,"d":"12.29"}]
["天沟",3.6,1.1,1,3.96]
["阁楼东外墙",9.9,1.4,1,13.86]
["阁楼西斜屋面",6.72,6.35,1,{"v":42.672,"d":"42.67"}]
["阁楼平台",8,7,1,{"v":56,"d":"56.00"}]
["石墩①",0.51,0.51,-40,{"v":-10.404,"d":"-10.40"}]
["石墩②",1.5,0.38,40,{"v":22.8,"d":"22.80"}]
["A31-401、901"]
["东墙",2.05,33,1,67.65]
["东墙平台",4.1,2,1,{"v":8.2,"d":"8.20"}]
["A31-801"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["北房东墙",2.4,6.5,1,{"v":15.6,"d":"15.60"}]
["空调板",1.86,1,1,1.86]
["北房北墙",3.7,6.5,1,24.05]
["窗",1.67,2,-1,-3.34]
["南房东墙",3,6.5,1,{"v":19.5,"d":"19.50"}]
["A34-1-901"]
["南房采光井",4.15,6.5,1,{"v":26.975,"d":"26.98"}]
["北房北墙",3.2,6.5,1,{"v":20.8,"d":"20.80"}]
["窗",2.13,1.6,-2,{"v":-6.816,"d":"-6.82"}]
["A34-1-1003"]
["东北房北墙",2.77,6.5,1,{"v":18.005,"d":"18.01"}]
["窗",1.44,1.83,-2,{"v":-5.2704,"d":"-5.27"}]
["飘窗顶",1.8,1,1,{"v":1.8,"d":"1.80"}]
["西北房北墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["窗",2.37,1.63,-2,{"v":-7.7262,"d":"-7.73"}]
["A2-3-508"]
["北房北墙",3.35,6.5,1,{"v":21.775,"d":"21.78"}]
["窗",1.87,1.78,-2,{"v":-6.6572,"d":"-6.66"}]
["飘窗顶",1.55,1,1,1.55]
["B1-1-301"]
["南房南墙",2.76,6.5,1,17.94]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["客厅东墙",3.45,6.5,1,{"v":22.425,"d":"22.43"}]
["B1-2-303"]
["北房北墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["西南房飘窗",2.46,6.5,1,15.99]
["飘窗",1.83,1.45,-1,{"v":-2.6535,"d":"-2.65"}]
["飘窗顶",1.45,1,1,1.45]
["东南房飘窗",3.38,6.5,1,21.97]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["B5-4-607"]
["北天沟",3.97,1.2,1,{"v":4.764,"d":"4.76"}]
["南天沟",3.97,1.2,1,{"v":4.764,"d":"4.76"}]
["阁楼西墙斜面",2.77,2.5,1,{"v":6.925,"d":"6.93"}]
["楼顶平台",8.3,5,1,{"v":41.5,"d":"41.50"}]
["石墩①",0.51,0.51,-22,{"v":-5.7222,"d":"-5.72"}]
["石墩②",1.5,0.38,22,12.54]
["北天沟",7.75,1.2,1,{"v":9.3,"d":"9.30"}]
["阁楼北斜屋面",6.72,6.35,1,{"v":42.672,"d":"42.67"}]
["东天沟",7,2,1,{"v":14,"d":"14.00"}]
["烟道",{"v":0.6232,"d":"0.62"},{"v":1.022,"d":"1.02"},1,{"v":0.6369104,"d":"0.64"}]
["北房北墙",3.2,3,1,{"v":9.6,"d":"9.60"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["南房南墙",3.4,3,1,{"v":10.2,"d":"10.20"}]
["窗户①",0.6,1.87,-1,{"v":-1.122,"d":"-1.12"}]
["窗户②",1.15,1.87,-1,{"v":-2.1505,"d":"-2.15"}]
["南房东墙",4.3,3,1,{"v":12.9,"d":"12.90"}]
["南北天沟",7.75,1.2,2,{"v":18.6,"d":"18.60"}]
["B11-1-102"]
["北房顶面",2.5,0.5,2,{"v":2.5,"d":"2.50"}]
["北外墙侧面",4.2,1,1,{"v":4.2,"d":"4.20"}]
["北外墙",2.5,3,1,{"v":7.5,"d":"7.50"}]
["B16-3-406"]
["西墙",2.65,21,1,55.65]
["西墙平台",4.2,2,1,{"v":8.4,"d":"8.40"}]
["西南房南墙",3.37,3,1,10.11]
["西南房飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["东南房南墙",2.77,3,1,8.31]
["窗",0.74,1.82,-2,{"v":-2.6936,"d":"-2.69"}]
["B20-1-601"]
["阁楼西墙斜面",2.77,2.5,1,{"v":6.925,"d":"6.93"}]
["阁楼楼面",3.7,3.4,1,12.58]
["石墩1",0.51,0.51,-6,{"v":-1.5606,"d":"-1.56"}]
["石墩2",1.5,0.38,6,3.42]
["楼梯道楼面",2,2,1,{"v":4,"d":"4.00"}]
["北天沟",9.3,2.5,1,23.25]
["客厅东墙",4.35,3,1,13.05]
["北房北墙",2.49,3,1,7.47]
["窗",1.8,1.5,-1,{"v":-2.7,"d":"-2.70"}]
["飘窗顶",1.5,1,1,{"v":1.5,"d":"1.50"}]
["B21-1-302"]
["北墙",2.36,6.5,1,15.34]
["窗",0.74,1.82,-2,{"v":-2.6936,"d":"-2.69"}]
["西北房飘窗",3.2,6.5,1,{"v":20.8,"d":"20.80"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["C3-3-2006"]
["阳台顶",4.73,1.92,1,{"v":9.0816,"d":"9.08"}]
["阁楼西墙",4.2,2,1,{"v":8.4,"d":"8.40"}]
["南天沟",4.73,0.82,2,{"v":7.7572,"d":"7.76"}]
["北天沟",4.73,0.82,2,{"v":7.7572,"d":"7.76"}]
["阁楼北斜屋面",6.72,6.35,1,{"v":42.672,"d":"42.67"}]
["阁楼南斜屋面",6.72,6.35,1,{"v":42.672,"d":"42.67"}]
["烟道",{"v":1.2,"d":"1.20"},{"v":1,"d":"1.00"}]
["阁楼南房西墙",4.95,2.75,1,{"v":13.6125,"d":"13.61"}]
["C6-3-1305"]
["北房北墙",2.72,6.5,1,17.68]
["北飘窗",1.84,1.76,-2,{"v":-6.4768,"d":"-6.48"}]
["飘窗顶",1.76,1,1,1.76]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["窗",1.8,1.76,-2,{"v":-6.336,"d":"-6.34"}]
["C9-1-2203"]
["北房北墙",3.2,3,1,{"v":9.6,"d":"9.60"}]
["北房飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["南房南墙",3.36,3,1,10.08]
["南房飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["C6-2-1203"]
["北房北墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["C8-1-302"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["客厅南墙外平台",1.85,0.5,1,{"v":0.925,"d":"0.93"}]
["C9-2-1004"]
["北房北墙",3.05,6.5,1,{"v":19.825,"d":"19.83"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["烟道",{"v":0.6232,"d":"0.62"},{"v":1.022,"d":"1.02"},1,{"v":0.6369104,"d":"0.64"}]
["C9-2-2106"]
["西南房南墙",3.37,6.5,1,{"v":21.905,"d":"21.91"}]
["南飘窗",1.75,1.35,-1,{"v":-2.3625,"d":"-2.36"}]
["飘窗顶",1.75,1,1,1.75]
["西北房北墙",3.37,6.5,1,{"v":21.905,"d":"21.91"}]
["北飘窗",1.75,1.35,-1,{"v":-2.3625,"d":"-2.36"}]
["飘窗顶",1.75,1,1,1.75]
["A3-1-601"]
["南墙",3.36,3,1,10.08]
["南墙飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["C13-2-1104"]
["客厅北墙①",2.95,2,1,{"v":5.9,"d":"5.90"}]
["客厅北墙②",1,1,1,{"v":1,"d":"1.00"}]
["北房间北墙",3.4,3,1,{"v":10.2,"d":"10.20"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["阁楼北房间北墙",2.4,3,1,{"v":7.2,"d":"7.20"}]
["阁楼南房南墙",2.5,3,1,{"v":7.5,"d":"7.50"}]
["阁楼南房西墙斜面",4.6,1.85,1,8.51]
["楼顶平台",5.8,5.5,1,{"v":31.9,"d":"31.90"}]
["石墩①",0.51,0.51,-24,{"v":-6.2424,"d":"-6.24"}]
["石墩②",1.5,0.38,24,13.68]
["楼顶北平台",6,3.3,1,{"v":19.8,"d":"19.80"}]
["石墩1",0.51,0.51,-12,{"v":-3.1212,"d":"-3.12"}]
["石墩2",1.5,0.38,12,6.84]
["烟道",{"v":0.6232,"d":"0.62"},{"v":1.022,"d":"1.02"},1,{"v":0.6369104,"d":"0.64"}]
["北天沟1",4.5,3.5,2,{"v":31.5,"d":"31.50"}]
["北天沟2",4.2,1,1,{"v":4.2,"d":"4.20"}]
["阁楼南斜屋面",5.5,6.5,1,35.75]
["阁楼北斜屋面",5.5,6.5,1,35.75]
["南天沟1",{"v":4,"d":"4.0"},3,1,{"v":12,"d":"12.00"}]
["南天沟2",{"v":4,"d":"4.0"},1,1,{"v":4,"d":"4.00"}]
["C14-1001"]
["南房南墙",3.4,3,1,{"v":10.2,"d":"10.20"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["南房西墙",4.8,6.5,1,{"v":31.2,"d":"31.20"}]
["北房北墙",3.4,3,1,{"v":10.2,"d":"10.20"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["北房北墙",2.8,6.5,1,{"v":18.2,"d":"18.20"}]
["窗",1.6,2.4,-1,-3.84]
["客厅东墙",2.05,33,1,67.65]
["客厅北墙",3.7,6.5,1,24.05]
["空调板",1.86,1,1,1.86]
["C15-701"]
["阳台",0.84,3,1,2.52]
["南房南墙",3.38,3,1,10.14]
["南房飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["C16-902"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.7,1.8,-1,-3.06]
["飘窗顶",1.7,1,1,{"v":1.7,"d":"1.70"}]
["东南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.7,1.8,-1,-3.06]
["飘窗顶",1.7,1,1,{"v":1.7,"d":"1.70"}]
["楼面①",10.4,6.5,1,{"v":67.6,"d":"67.60"}]
["楼面②",11.2,5,1,{"v":56,"d":"56.00"}]
["楼面③",3.6,2.4,1,8.64]
["外墙",5.17,3,1,15.51]
["地面",5.17,2.4,1,{"v":12.408,"d":"12.41"}]
["A3-3-506"]
["南房南墙",3.4,6.5,1,{"v":22.1,"d":"22.10"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["北房北墙",2.55,6.5,1,{"v":16.575,"d":"16.58"}]
["飘窗",1.86,1.75,-1,{"v":-3.255,"d":"-3.26"}]
["飘窗顶",1.86,1,1,1.86]
["A3-4-607"]
["阁楼北斜屋面",6.72,6.35,1,{"v":42.672,"d":"42.67"}]
["阁楼南斜屋面",6.72,6.35,1,{"v":42.672,"d":"42.67"}]
["A4-2-603"]
["南天沟",7.24,2.5,1,{"v":18.1,"d":"18.10"}]
["天台",8.5,7.5,1,63.75]
["石墩1",0.51,0.51,-48,{"v":-12.4848,"d":"-12.48"}]
["石墩2",1.5,0.38,48,27.36]
["C18-4-510"]
["阁楼北斜屋面",{"v":6.6,"d":"6.60"},6.35,1,41.91]
["阁楼南斜屋面",{"v":6.6,"d":"6.60"},6.35,1,41.91]
["天沟",4.2,1.5,1,{"v":6.3,"d":"6.30"}]
["西南房西墙",4.3,3,1,{"v":12.9,"d":"12.90"}]
["石墩平面",1,0.38,28,10.64]
["总计","户数",42]

{"sheet":"紫竹园","index":2,"n_rows":85,"n_cols":7,"rows_kept":85,"merged":[[0,2,0,6],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[84,4,84,6]]}
[null,null,"紫竹园"]
[null,null,"维修部位","长度","宽度（高度）","计量","总量"]
[]
[null,null,"3-2-606室"]
[null,null,"天窗斜顶",6,4.87,1,{"$f":"D5*E5*F5","v":29.22}]
[null,null,"南天沟",3.71,1,1,3.71]
[null,null,"3-1-601室"]
[null,null,"西南房斜顶",3.15,4.03,1,{"v":12.6945,"d":"12.69"}]
[null,null,"4-1-602室"]
[null,null,"阳光房",2.35,3.55,1,{"$f":"D10*E10*F10","v":{"v":8.3425,"d":"8.34"}}]
[null,null,"2-1-602室"]
[null,null,"阁楼平台",2.3,2,1,{"v":4.6,"d":"4.60"}]
[null,null,"平台北墙",0.9,3,1,{"v":2.7,"d":"2.70"}]
[null,null,"楼顶平台",5,6.5,1,{"v":32.5,"d":"32.50"}]
[null,null,"4-4-608室"]
[null,null,"楼面",3.7,6.2,1,{"$f":"D16*E16*F16","v":22.94}]
[null,null,"东天沟",4,1.2,1,{"v":4.8,"d":"4.80"}]
[null,null,"西天沟",4,1.2,1,{"v":4.8,"d":"4.80"}]
[null,null,"4-5-109室"]
[null,null,"北房北墙",2.8,3,1,{"$f":"D20*E20*F20","v":{"v":8.399999999999999,"d":"8.40"}}]
[null,null,"窗户",1.55,1.42,-1,{"v":-2.201,"d":"-2.20"}]
[null,null,"窗沿",1.55,0.2,4,{"v":1.2400000000000002,"d":"1.24"}]
[null,null,"空调板",1.5,1,2,{"v":3,"d":"3.00"}]
[null,null,"7-1-1603室"]
[null,null,"北房西墙",3.4,6,1,{"$f":"D25*E25*F25","v":{"v":20.4,"d":"20.40"}}]
[null,null,"窗户",2.35,1.56,-1,{"v":-3.6660000000000004,"d":"-3.67"}]
[null,null,"窗沿",2.35,0.2,4,{"v":1.8800000000000001,"d":"1.88"}]
[null,null,"7-1-1701室"]
[null,null,"楼道西墙",3.59,3,1,{"$f":"D29*E29","v":10.77}]
[null,null,"7-2-904室"]
[null,null,"北房北墙",3.25,6,1,{"$f":"D31*E31*F31","v":{"v":19.5,"d":"19.50"}}]
[null,null,"窗",1.8,1.43,-2,{"v":-5.148,"d":"-5.15"}]
[null,null,"窗沿",1.8,0.2,4,{"v":1.4400000000000002,"d":"1.44"}]
[null,null,"10-204室"]
[null,null,"南房南墙",1.4,6,1,{"$f":"D35*E35*F35","v":{"v":8.399999999999999,"d":"8.40"}}]
[null,null,"平台西墙",1,6,1,{"v":6,"d":"6.00"}]
[null,null,"平台",1,2.8,1,{"v":2.8,"d":"2.80"}]
[null,null,"12-1806室"]
[null,null,"楼顶平台1",3.1,2.92,1,{"$f":"D39*E39*F39","v":{"v":9.052,"d":"9.05"}}]
[null,null,"楼顶平台2",6.38,7.2,1,{"v":45.936,"d":"45.94"}]
[null,null,"楼顶平台3",4.5,1.42,1,6.39]
[null,null,"楼顶平台围墙1",{"$f":"1.85+2.05+2.92+4.1+5.1+1.28+7.2","v":24.5},2.35,1,{"v":57.575,"d":"57.58"}]
[null,null,"楼顶平台围墙2",2.2,2.35,1,{"v":5.170000000000001,"d":"5.17"}]
[null,null,"15-1803室"]
[null,null,"楼顶平台1",5.83,3.6,1,{"$f":"D45*E45*F45","v":{"v":20.988,"d":"20.99"}}]
[null,null,"楼顶平台2",6.25,5.7,1,{"v":35.625,"d":"35.63"}]
[null,null,"楼顶平台3",1.95,3.68,1,{"v":7.176,"d":"7.18"}]
[null,null,"楼顶平台围墙",2,{"$f":"5+1.2+5.1+0.4","v":11.700000000000001},1,{"v":23.400000000000002,"d":"23.40"}]
[null,null,"3-3-109室"]
[null,null,"卫生间东墙",3,2.46,1,{"$f":"D50*E50*F50","v":7.38}]
[null,null,"采光井",2.48,3,1,{"v":7.4399999999999995,"d":"7.44"}]
[null,null,"挡板",2.1,2.48,1,{"v":5.208,"d":"5.21"}]
[null,null,"南墙",1.4,3,1,{"v":4.199999999999999,"d":"4.20"}]
[null,null,"空调平台",1.5,1,1,{"v":1.5,"d":"1.50"}]
[null,null,"侧墙",0.96,3,1,2.88]
[null,null,"17-1-301室"]
[null,null,"客厅东墙",4,3,1,{"$f":"D57*E57*F57","v":{"v":12,"d":"12.00"}}]
[null,null,"窗",2.35,1.65,-1,{"v":-3.8775,"d":"-3.88"}]
[null,null,"窗沿",2.35,0.2,4,{"v":1.8800000000000001,"d":"1.88"}]
[null,null,"东墙平台",10,1.5,1,{"v":15,"d":"15.00"}]
[null,null,"4-3-506室"]
[null,null,"南房顶",4.4,2.75,1,{"$f":"D62*E62*F62","v":{"v":12.100000000000001,"d":"12.10"}}]
[null,null,"伸缩缝",1.4,0.5,1,{"v":0.7,"d":"0.70"}]
[null,null,"17-1-1201室"]
[null,null,"东房东墙",{"$f":"0.62+1.57","v":2.19},3,1,6.57]
[null,null,"平台",2.19,0.7,1,{"v":1.533,"d":"1.53"}]
[null,null,"平台围墙1",3,0.7,1,{"v":2.0999999999999996,"d":"2.10"}]
[null,null,"平台围墙2",3,1.2,1,{"v":3.5999999999999996,"d":"3.60"}]
[null,null,"9-1-1802室"]
[null,null,"客厅南墙外平台",6,0.35,1,{"$f":"D70*E70*F70","v":{"v":2.0999999999999996,"d":"2.10"}}]
[null,null,"客厅南墙",2.4,4.5,1,{"v":10.799999999999999,"d":"10.80"}]
[null,null,"窗",1.35,1.4,-1,-1.89]
[null,null,"窗沿",0.2,1.4,4,{"v":1.1199999999999999,"d":"1.12"}]
[null,null,"17-1-1501室"]
[null,null,"南房南墙",1.4,6,1,{"$f":"D75*E75*F75","v":{"v":8.399999999999999,"d":"8.40"}}]
[null,null,"平台西墙",1,6,1,{"v":6,"d":"6.00"}]
[null,null,"平台",1,2.8,1,{"v":2.8,"d":"2.80"}]
[null,null,"南房东墙",7.2,6,1,{"v":43.2,"d":"43.20"}]
[null,null,"2-2-602室"]
[null,null,"北房斜顶窗户",1.15,0.86,1,{"$f":"D80*E80*F80","v":{"v":0.9889999999999999,"d":"0.99"}}]
[null,null,"17-2-1805室"]
[null,null,"楼顶南围墙",3.55,3.97,1,{"v":14.0935,"d":"14.09"}]
[null,null,"楼顶南围墙",1.15,1.55,-2,{"v":-3.565,"d":"-3.57"}]
[null,null,"楼顶南侧墙",1.55,1.55,1,{"v":2.4025000000000003,"d":"2.40"}]
[null,null,"总计","户数",20]